Here is send you all midi signals from one of our midi files. With this midifile i control our „light controller and our A&H SQ 5.

The thing is, that i need the full signal from the midi file to the „light controler“ and only the program changes to the „SQ5“. But i don´t need all of the PC in the SQ 5, only the PC between 79 and 89. And at the end every of this PC between 79 and 89 shoud be a differnt CC after turnslate. I hope you can follow me?

The signal list from the Capture Midi (Bome Box)







